

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/04/13 00:10:16 |
| Type: | Unframed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.00.1000.17 |
| Test Start Time | 2025/04/13 00:07:08 |
| Test End Time | 2025/04/13 00:10:16 |
| Test Duration | 00:01:00 |
| Pass/Fail Verdict | PASS |
| Module Type | 1,1,3 - PassiveCopper 1,1,4 - PassiveCopper |
| Module Version | 1,1,3 - CMIS 5.0 1,1,4 - CMIS 5.0 |
| Serial Number | 1,1,3 - 57ADUAD233140Z 1,1,4 - 57ADUAD233140Z |

# Transceiver DOM (Digital Optical Monitoring) - BERT

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1,1,3** |  |  |  |  |  |  |  |  |  |  |
| **Manufactuer** | TE Connectivity | **Model** | 2369405-2 | **Mfg Revision** | 11 |  |  |  |  |  |
| **Type** | PassiveCopper | **SN** | 57ADUAD233140Z | **Firmware Revision** |  |  |  |  |  |  |
| **MSA** | CMIS 5.0 | **Date Code(YYMMDDLL)** | 230904 | **Hardware Revision** |  |  |  |  |  |  |
| **Media Tech** | Copper cable unequalized | **Media Connector** | No separable connector |  |  |  |  |  |  |  |
| **Cable Lenth** | 1.0 m | **Identifier Type** | OSFP |  |  |  |  |  |  |  |
| **Reported Power Class** | 1 | **Reported Max Power** | 0.250000 W |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **Modlue** | **High Alarm** | **High Warn** | **Low Warn** | **Low Alarm** |  |  |  |  |  |  |
| **Temperature** | -0.001 C | -0.001 C | -0.001 C | -0.001 C |  |  |  |  |  |  |
| **Supply Voltage** | -0.000 V | -0.000 V | -0.000 V | -0.000 V |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **Lane Limits** | **High Alarm** | **High Warn** | **Low Warn** | **Low Alarm** |  |  |  |  |  |  |
| **Tx Optical Power** | -40.00 dBm | -40.00 dBm | -40.00 dBm | -40.00 dBm |  |  |  |  |  |  |
| **Rx Optical Power** | -40.00 dBm | -40.00 dBm | -40.00 dBm | -40.00 dBm |  |  |  |  |  |  |
| **Tx Bias Current** | -40.00 dBm | -40.00 dBm | -40.00 dBm | -40.00 dBm |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **Host Lane** | **Port** | **Data Path State** | **Tx LOS** | **Tx CDR LOL** | **Media Lane** | **Tx Optical Power** | **Tx Bias Cureent** | **Rx Optical Power** | **Rx LOS** | **Rx CDR LOL** |
| 1 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 2 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 3 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 4 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 5 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 6 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 7 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 8 | 3.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1,1,4** |  |  |  |  |  |  |  |  |  |  |
| **Manufactuer** | TE Connectivity | **Model** | 2369405-2 | **Mfg Revision** | 11 |  |  |  |  |  |
| **Type** | PassiveCopper | **SN** | 57ADUAD233140Z | **Firmware Revision** |  |  |  |  |  |  |
| **MSA** | CMIS 5.0 | **Date Code(YYMMDDLL)** | 230904 | **Hardware Revision** |  |  |  |  |  |  |
| **Media Tech** | Copper cable unequalized | **Media Connector** | No separable connector |  |  |  |  |  |  |  |
| **Cable Lenth** | 1.0 m | **Identifier Type** | OSFP |  |  |  |  |  |  |  |
| **Reported Power Class** | 1 | **Reported Max Power** | 0.250000 W |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **Modlue** | **High Alarm** | **High Warn** | **Low Warn** | **Low Alarm** |  |  |  |  |  |  |
| **Temperature** | -0.001 C | -0.001 C | -0.001 C | -0.001 C |  |  |  |  |  |  |
| **Supply Voltage** | -0.000 V | -0.000 V | -0.000 V | -0.000 V |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **Lane Limits** | **High Alarm** | **High Warn** | **Low Warn** | **Low Alarm** |  |  |  |  |  |  |
| **Tx Optical Power** | -40.00 dBm | -40.00 dBm | -40.00 dBm | -40.00 dBm |  |  |  |  |  |  |
| **Rx Optical Power** | -40.00 dBm | -40.00 dBm | -40.00 dBm | -40.00 dBm |  |  |  |  |  |  |
| **Tx Bias Current** | -40.00 dBm | -40.00 dBm | -40.00 dBm | -40.00 dBm |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **Host Lane** | **Port** | **Data Path State** | **Tx LOS** | **Tx CDR LOL** | **Media Lane** | **Tx Optical Power** | **Tx Bias Cureent** | **Rx Optical Power** | **Rx LOS** | **Rx CDR LOL** |
| 1 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 2 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 3 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 4 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 5 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 6 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 7 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |
| 8 | 4.1 | 0 | No | No | 0 | -40.00 dBm | 0.000 mA | -40.00 dBm | No | No |

# CMIS Applicatio Select

|  |  |
| --- | --- |
| 1,1,3 |  |
| Current AppSel | 0 |

Available Applications

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **App** | **Host Side** | | | | | | **Line Side Media** | | | | |
|  | **Interface** | **Lane Speed (G bit/s)** | **Modulation** | **Lane Groups** | **Lanes** | **ID (HEex)** | **Interface** | **Lane Speed (G bit/s)** | **Lane Groups** | **Lanes** | **ID (Hex)** |
| 1 | 800GBASE-CR8 | 106 | PAM4 | 1 | 8 | 73 | PassiveCopper |  | 0 | 8 | 1 |
| 2 | 400GBASE-CR4 | 106 | PAM4 | 2 | 4 | 72 | PassiveCopper |  | 0 | 4 | 1 |
| 3 | 200GBASE-CR2 | 106 | PAM4 | 4 | 2 | 71 | PassiveCopper |  | 0 | 2 | 1 |
| 4 | 100GBASE-CR1 | 106 | PAM4 | 8 | 1 | 70 | PassiveCopper |  | 0 | 1 | 1 |
| 5 | 400GBASE-CR8 | 53 | PAM4 | 1 | 8 | 29 | PassiveCopper |  | 0 | 8 | 1 |
| 6 | 200GBASE-CR4 | 53 | PAM4 | 2 | 4 | 28 | PassiveCopper |  | 0 | 4 | 1 |
| 7 | 100GBASE-CR2 | 53 | PAM4 | 4 | 2 | 27 | PassiveCopper |  | 0 | 2 | 1 |
| 8 | 50GBASE-CR | 53 | PAM4 | 8 | 1 | 24 | PassiveCopper |  | 0 | 1 | 1 |

Preview of Auto selected applications

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Host Port Mode** | **Mod** | **Lane Groups** | **Lanes** | **AppSel** | **Link** | **Host Electrical** | **Lane Groups** | **Lanes** | **Note** |

|  |  |
| --- | --- |
| 1,1,4 |  |
| Current AppSel | 0 |

Available Applications

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **App** | **Host Side** | | | | | | **Line Side Media** | | | | |
|  | **Interface** | **Lane Speed (G bit/s)** | **Modulation** | **Lane Groups** | **Lanes** | **ID (HEex)** | **Interface** | **Lane Speed (G bit/s)** | **Lane Groups** | **Lanes** | **ID (Hex)** |
| 1 | 800GBASE-CR8 | 106 | PAM4 | 1 | 8 | 73 | PassiveCopper |  | 0 | 8 | 1 |
| 2 | 400GBASE-CR4 | 106 | PAM4 | 2 | 4 | 72 | PassiveCopper |  | 0 | 4 | 1 |
| 3 | 200GBASE-CR2 | 106 | PAM4 | 4 | 2 | 71 | PassiveCopper |  | 0 | 2 | 1 |
| 4 | 100GBASE-CR1 | 106 | PAM4 | 8 | 1 | 70 | PassiveCopper |  | 0 | 1 | 1 |
| 5 | 400GBASE-CR8 | 53 | PAM4 | 1 | 8 | 29 | PassiveCopper |  | 0 | 8 | 1 |
| 6 | 200GBASE-CR4 | 53 | PAM4 | 2 | 4 | 28 | PassiveCopper |  | 0 | 4 | 1 |
| 7 | 100GBASE-CR2 | 53 | PAM4 | 4 | 2 | 27 | PassiveCopper |  | 0 | 2 | 1 |
| 8 | 50GBASE-CR | 53 | PAM4 | 8 | 1 | 24 | PassiveCopper |  | 0 | 1 | 1 |

Preview of Auto selected applications

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Host Port Mode** | **Mod** | **Lane Groups** | **Lanes** | **AppSel** | **Link** | **Host Electrical** | **Lane Groups** | **Lanes** | **Note** |

# BERT Result Summary

|  |  |  |
| --- | --- | --- |
| **Bit Error Ratio** | **1,1,3** | **1,1,4** |
| **BER Threshold** | 2.400000e-04 | 2.400000e-04 |
| **Pre-BER Pass/Fail Verdict** | PASS | PASS |

# BERT Statistics

Port - 1,1,3

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Physical Lane** | **Pattern Lock** | **Pattern Transmitted** | **Pattern Received** | **Bits Send** | **Bits Received** | **Bit Error Received** | **Bit Error Ratio** |
| **Totals** | lock | 11Q | 11Q | 55664699487280.0 | 55664699493120.0 | 3390.0 | 1.945590e-09 |
| **0** | lock | 11Q | 11Q | 6902091187840 | 6902091187200 | 185 | 1.072500e-10 |
| **1** | lock | 11Q | 11Q | 6902091187840 | 6902091189120 | 381 | 2.203000e-10 |
| **2** | lock | 11Q | 11Q | 6958137387280 | 6958137386880 | 122 | 7.020000e-11 |
| **3** | lock | 11Q | 11Q | 6958137387200 | 6958137388800 | 67 | 3.850000e-11 |
| **4** | lock | 11Q | 11Q | 6958137387280 | 6958137388800 | 919 | 5.283000e-10 |
| **5** | lock | 11Q | 11Q | 6958137387200 | 6958137388800 | 767 | 4.400000e-10 |
| **6** | lock | 11Q | 11Q | 7013983781200 | 7013983779840 | 843 | 4.806000e-10 |
| **7** | lock | 11Q | 11Q | 7013983781440 | 7013983783680 | 106 | 6.044000e-11 |

Port - 1,1,4

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Physical Lane** | **Pattern Lock** | **Pattern Transmitted** | **Pattern Received** | **Bits Send** | **Bits Received** | **Bit Error Received** | **Bit Error Ratio** |
| **Totals** | lock | 11Q | 11Q | 56225488232640.0 | 56225488235520.0 | 37588.0 | 2.142458e-08 |
| **0** | lock | 11Q | 11Q | 7014713863200 | 7014713863680 | 81 | 4.617000e-11 |
| **1** | lock | 11Q | 11Q | 7014713863200 | 7014713863680 | 74 | 4.220000e-11 |
| **2** | lock | 11Q | 11Q | 7014713863040 | 7014713863680 | 1210 | 6.898000e-10 |
| **3** | lock | 11Q | 11Q | 7014713863360 | 7014713863680 | 50 | 2.853000e-11 |
| **4** | lock | 11Q | 11Q | 7014713863280 | 7014713863680 | 23635 | 1.347000e-08 |
| **5** | lock | 11Q | 11Q | 7014713863280 | 7014713863680 | 8266 | 4.714000e-09 |
| **6** | lock | 11Q | 11Q | 7014713863200 | 7014713863680 | 4103 | 2.339000e-09 |
| **7** | lock | 11Q | 11Q | 7122491190080 | 7122491189760 | 169 | 9.488000e-11 |

# FEC Result Summary

No FEC Result Summary data available.

# PCS Lane Statistics

No PCS Lane Statistics data available.

# L2 Traffic Test Summary

No L2 Traffic Test Summary data available.

# Port Statistics - BERT

|  |  |  |
| --- | --- | --- |
| **Port Statistics** | **Port 1,1,3** | **Port 1,1,4** |
| link | link up | link up |
| transmitState | 0 | 0 |
| lineSpeed | 800000 | 800000 |
| bertBitsSent | 55216729503760 | 55204684766000 |
| bertBitsReceived | 55216729509120 | 55204684769280 |
| bertBitErrorsReceived | 3349 | 36998 |
| bertBitErrorRatio | 6.070000e-11 | 6.700000e-10 |
| centralTemperature | 42 | 42 |
| portTemperature | 61 | 58 |
| pcpuFpgaTemperature | 35 | 35 |
| bertTransmitDuration | 00:02:00.094812700 | 00:01:59.975327260 |
| encoding | PAM4 106G | PAM4 106G |
| transceiverTemp | 0 | 0 |
| transceiverVoltage | 0 | 0 |
| minLatency | 0 | 0 |
| averageLatency | 0 | 0 |
| maxLatency | 0 | 0 |