|  |  |
| --- | --- |
|  |  |

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/07/15 17:43:21 |
| Type: | Framed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.80.8001.4 |
| Test Start Time | 2025/07/15 17:42:05 |
| Test End Time | 2025/07/15 17:43:20 |
| Test Duration | 00:00:10 |
| Pass/Fail Verdict | PASS |
| Module Type |  |
| Module Version |  |
| Serial Number |  |

# L2 Traffic Test Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Size** | **Tx Count** | **Rx Count** | **Loss Count** | **Loss %** |
| **128** | 1721748872 | 1721748872 | 0 | 0.0 |

# Port Statistics - 128

|  |  |  |
| --- | --- | --- |
| **Port Statistics** | **Port 1,1,1** | **Port 1,1,2** |
| link | link up | link up |
| lineSpeed | 100000 | 100000 |
| transmitDuration | 00:00:10.193088036 | 00:00:10.192418605 |
| framesSent | 860902706 | 860846166 |
| framesReceived | 860902706 | 860846166 |
| fragments | 0 | 0 |
| undersize | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 |
| flowControlFrames | 0 | 0 |
| bitsSent | 881564370944 | 881506473984 |
| bitsReceived | 881506473984 | 881564370944 |
| pcsSyncErrorsReceived | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 |
| fecTotalCodewords | 253602461 | 253494851 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 |
| l1BitsSent | 1019308803904 | 1019241860544 |
| l1BitsReceived | 1019241860544 | 1019308803904 |
| transceiverTemp | 0 | 0 |
| transceiverVoltage | 0 | 0 |
| minLatency | 85899018240 | 310047 |
| averageLatency | 5823720615 | 310052 |
| maxLatency | 85899035865 | 310055 |
| Loss\_Frames | 0 | 0 |
| Loss% | 0.0 | 0.0 |