|  |  |
| --- | --- |
|  |  |

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/07/16 11:42:54 |
| Type: | Framed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.80.8001.4 |
| Test Start Time | 2025/07/16 11:40:17 |
| Test End Time | 2025/07/16 11:42:53 |
| Test Duration | 00:00:30 |
| Pass/Fail Verdict | PASS |
| Module Type |  |
| Module Version |  |
| Serial Number |  |

# L2 Traffic Test Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Size** | **Tx Count** | **Rx Count** | **Loss Count** | **Loss %** |
| **64** | 8985347647 | 8985347647 | 0 | 0.0 |

# Port Statistics - 64

|  |  |  |
| --- | --- | --- |
| **Port Statistics** | **Port 1,1,1** | **Port 1,1,2** |
| link | link up | link up |
| lineSpeed | 100000 | 100000 |
| transmitDuration | 00:00:30.191085217 | 00:00:30.190450965 |
| framesSent | 4492721015 | 4492626632 |
| framesReceived | 4492721015 | 4492626632 |
| fragments | 0 | 0 |
| undersize | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 |
| flowControlFrames | 0 | 0 |
| bitsSent | 2300273159680 | 2300224835584 |
| bitsReceived | 2300224835584 | 2300273159680 |
| pcsSyncErrorsReceived | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 |
| fecTotalCodewords | 645031929 | 644924661 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 |
| l1BitsSent | 3019108522080 | 3019045096704 |
| l1BitsReceived | 3019045096704 | 3019108522080 |
| transceiverTemp | 0 | 0 |
| transceiverVoltage | 0 | 0 |
| minLatency | 225512960 | 85673820160 |
| averageLatency | 225515457 | 1754801421 |
| maxLatency | 225515472 | 85673830472 |
| Loss\_Frames | 0 | 0 |
| Loss% | 0.0 | 0.0 |