|  |  |
| --- | --- |
|  |  |

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/07/16 11:48:17 |
| Type: | Framed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.80.8001.4 |
| Test Start Time | 2025/07/16 11:45:15 |
| Test End Time | 2025/07/16 11:48:16 |
| Test Duration | 00:00:30 |
| Pass/Fail Verdict | PASS |
| Module Type |  |
| Module Version |  |
| Serial Number |  |

# L2 Traffic Test Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Size** | **Tx Count** | **Rx Count** | **Loss Count** | **Loss %** |
| **64** | 8988681866 | 8988681866 | 0 | 0.0 |

# Port Statistics - 64

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Port Statistics** | **Port 1,1,61** | **Port 1,1,62** | **Port 1,1,63** | **Port 1,1,64** |
| link | link up | link up | link up | link up |
| lineSpeed | 50000 | 50000 | 50000 | 50000 |
| transmitDuration | 00:00:30.202799114 | 00:00:30.202272454 | 00:00:30.201729356 | 00:00:30.201083348 |
| framesSent | 2247232077 | 2247192891 | 2247152482 | 2247104416 |
| framesReceived | 2247104416 | 2247152482 | 2247192891 | 2247232077 |
| fragments | 0 | 0 | 0 | 0 |
| undersize | 0 | 0 | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 | 0 | 0 |
| flowControlFrames | 0 | 0 | 0 | 0 |
| bitsSent | 1150582823424 | 1150562760192 | 1150542070784 | 1150517460992 |
| bitsReceived | 1150542070784 | 1150517460992 | 1150582823424 | 1150562760192 |
| pcsSyncErrorsReceived | 0 | 0 | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 | 0 | 0 |
| fecTotalCodewords | 323186997 | 323151060 | 323120888 | 323089405 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 | 0 | 0 |
| l1BitsSent | 1510139955744 | 1510113622752 | 1510086467904 | 1510054167552 |
| l1BitsReceived | 1510086467904 | 1510054167552 | 1510139955744 | 1510113622752 |
| transceiverTemp | 0 | 0 | 0 | 0 |
| transceiverVoltage | 0 | 0 | 0 | 0 |
| minLatency | 85898608640 | 85898608640 | 700455 | 676570 |
| averageLatency | 2016057005 | 1993335600 | 700459 | 676574 |
| maxLatency | 85898645510 | 85898669392 | 700467 | 676582 |
| Loss\_Frames | 127661 | 40409 | -40409 | -127661 |
| Loss% | 5.6808106873600846e-05 | 1.798198995815531e-05 | -1.798231331593278e-05 | -5.681133421794673e-05 |