|  |  |
| --- | --- |
|  |  |

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/07/16 15:19:02 |
| Type: | Framed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.80.8001.4 |
| Test Start Time | 2025/07/16 15:14:56 |
| Test End Time | 2025/07/16 15:19:02 |
| Test Duration | 00:00:30 |
| Pass/Fail Verdict | PASS |
| Module Type |  |
| Module Version |  |
| Serial Number |  |

# L2 Traffic Test Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Size** | **Tx Count** | **Rx Count** | **Loss Count** | **Loss %** |
| **64** | 8986892974 | 8986892974 | 0 | 0.0 |
| **1518** | 490742757 | 490742757 | 0 | 0.0 |

# Port Statistics - 64

|  |  |  |
| --- | --- | --- |
| **Port Statistics** | **Port 1,1,1** | **Port 1,1,2** |
| link | link up | link up |
| lineSpeed | 100000 | 100000 |
| transmitDuration | 00:00:30.196309490 | 00:00:30.195611303 |
| framesSent | 4493498435 | 4493394539 |
| framesReceived | 4493498435 | 4493394539 |
| fragments | 0 | 0 |
| undersize | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 |
| flowControlFrames | 0 | 0 |
| bitsSent | 2300671198720 | 2300618003968 |
| bitsReceived | 2300618003968 | 2300671198720 |
| pcsSyncErrorsReceived | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 |
| fecTotalCodewords | 644343382 | 644239488 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 |
| l1BitsSent | 3019630948320 | 3019561130208 |
| l1BitsReceived | 3019561130208 | 3019630948320 |
| transceiverTemp | 0 | 0 |
| transceiverVoltage | 0 | 0 |
| minLatency | 85898936320 | 335942 |
| averageLatency | 1998154777 | 335947 |
| maxLatency | 85899009965 | 335962 |
| Loss\_Frames | 0 | 0 |
| Loss% | 0.0 | 0.0 |

# Port Statistics - 1518

|  |  |  |
| --- | --- | --- |
| **Port Statistics** | **Port 1,1,1** | **Port 1,1,2** |
| link | link up | link up |
| lineSpeed | 100000 | 100000 |
| transmitDuration | 00:00:30.190832953 | 00:00:30.190155873 |
| framesSent | 245374130 | 245368627 |
| framesReceived | 245374130 | 245368627 |
| fragments | 0 | 0 |
| undersize | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 |
| flowControlFrames | 0 | 0 |
| bitsSent | 2979823434720 | 2979756606288 |
| bitsReceived | 2979756606288 | 2979823434720 |
| pcsSyncErrorsReceived | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 |
| fecTotalCodewords | 643539781 | 643433521 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 |
| l1BitsSent | 3019083295520 | 3019015586608 |
| l1BitsReceived | 3019015586608 | 3019083295520 |
| transceiverTemp | 0 | 0 |
| transceiverVoltage | 0 | 0 |
| minLatency | 85898936320 | 335942 |
| averageLatency | 9089018399 | 335949 |
| maxLatency | 85899009950 | 335965 |
| Loss\_Frames | 0 | 0 |
| Loss% | 0.0 | 0.0 |