|  |  |
| --- | --- |
|  |  |

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/07/17 00:30:30 |
| Type: | Framed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.80.8001.4 |
| Test Start Time | 2025/07/17 00:28:46 |
| Test End Time | 2025/07/17 00:30:29 |
| Test Duration | 00:00:30 |
| Pass/Fail Verdict | PASS |
| Module Type |  |
| Module Version |  |
| Serial Number |  |

# L2 Traffic Test Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Size** | **Tx Count** | **Rx Count** | **Loss Count** | **Loss %** |
| **64** | 17972080923 | 17972080923 | 0 | 0.0 |

# Port Statistics - 64

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Port Statistics** | **Port 1,1,1** | **Port 1,1,2** | **Port 1,1,3** | **Port 1,1,4** |
| link | link up | link up | link up | link up |
| lineSpeed | 100000 | 100000 | 100000 | 100000 |
| transmitDuration | 00:00:30.193956755 | 00:00:30.193426613 | 00:00:30.192838637 | 00:00:30.192161805 |
| framesSent | 4493148327 | 4493069436 | 4492981939 | 4492881221 |
| framesReceived | 4493148327 | 4493069436 | 4492981939 | 4492881221 |
| fragments | 0 | 0 | 0 | 0 |
| undersize | 0 | 0 | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 | 0 | 0 |
| flowControlFrames | 0 | 0 | 0 | 0 |
| bitsSent | 2300491943424 | 2300451551232 | 2300406752768 | 2300355185152 |
| bitsReceived | 2300451551232 | 2300491943424 | 2300355185152 | 2300406752768 |
| pcsSyncErrorsReceived | 0 | 0 | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 | 0 | 0 |
| fecTotalCodewords | 645869170 | 645736137 | 645636715 | 645541895 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 | 0 | 0 |
| l1BitsSent | 3019395675744 | 3019342660992 | 3019283863008 | 3019216180512 |
| l1BitsReceived | 3019342660992 | 3019395675744 | 3019216180512 | 3019283863008 |
| transceiverTemp | 0 | 0 | 36 | 36 |
| transceiverVoltage | 0 | 0 | 3.2446000000000002 | 3.2473999999999998 |
| minLatency | 869189120 | 85030092800 | 84982251520 | 917066240 |
| averageLatency | 869189232 | 1121398558 | 1060491594 | 917067171 |
| maxLatency | 869189247 | 85030156690 | 84982278752 | 917067175 |
| Loss\_Frames | 0 | 0 | 0 | 0 |
| Loss% | 0.0 | 0.0 | 0.0 | 0.0 |