|  |  |
| --- | --- |
|  |  |

Keysight Test Report

**PASS**

|  |  |
| --- | --- |
| Report Header: | Keysight Inc. |
| Report Date: | 2025/07/17 10:37:36 |
| Type: | Framed |

# SUMMARY

|  |  |
| --- | --- |
| IxOS Version | 10.80.8001.4 |
| Test Start Time | 2025/07/17 10:35:58 |
| Test End Time | 2025/07/17 10:37:36 |
| Test Duration | 00:00:30 |
| Pass/Fail Verdict | PASS |
| Module Type |  |
| Module Version |  |
| Serial Number |  |

# L2 Traffic Test Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Size** | **Tx Count** | **Rx Count** | **Loss Count** | **Loss %** |
| **64** | 17972598912 | 17972598912 | 0 | 0.0 |

# Port Statistics - 64

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Port Statistics** | **Port 1,1,1** | **Port 1,1,2** | **Port 1,1,3** | **Port 1,1,4** |
| link | link up | link up | link up | link up |
| lineSpeed | 100000 | 100000 | 100000 | 100000 |
| transmitDuration | 00:00:30.194899694 | 00:00:30.194317511 | 00:00:30.193693236 | 00:00:30.192954241 |
| framesSent | 4493288645 | 4493202011 | 4493109113 | 4492999143 |
| framesReceived | 4493202011 | 4493288645 | 4492999143 | 4493109113 |
| fragments | 0 | 0 | 0 | 0 |
| undersize | 0 | 0 | 0 | 0 |
| oversizeAndCrcErrors | 0 | 0 | 0 | 0 |
| vlanTaggedFramesRx | 0 | 0 | 0 | 0 |
| flowControlFrames | 0 | 0 | 0 | 0 |
| bitsSent | 2300563786240 | 2300519429632 | 2300471865856 | 2300415561216 |
| bitsReceived | 2300519429632 | 2300563786240 | 2300415561216 | 2300471865856 |
| pcsSyncErrorsReceived | 0 | 0 | 0 | 0 |
| pcsRemoteFaultsReceived | 0 | 0 | 0 | 0 |
| pcsLocalFaultsReceived | 0 | 0 | 0 | 0 |
| fecCorrectedCodewords | 0 | 0 | 0 | 0 |
| fecTotalCodewords | 649651810 | 649651810 | 649651810 | 649651809 |
| fecFrameLossRatio | 0.000000e+00 | 0.000000e+00 | 0.000000e+00 | 0.000000e+00 |
| fecUncorrectableCodewords | 0 | 0 | 0 | 0 |
| l1BitsSent | 3019489969440 | 3019431751392 | 3019369323936 | 3019295424096 |
| l1BitsReceived | 3019431751392 | 3019489969440 | 3019295424096 | 3019369323936 |
| transceiverTemp | 0 | 0 | 36 | 36 |
| transceiverVoltage | 0 | 0 | 3.2450999999999999 | 3.25 |
| minLatency | 869189120 | 85030092800 | 84982251520 | 917066240 |
| averageLatency | 869189231 | 1125379133 | 1063739773 | 917067176 |
| maxLatency | 869189247 | 85030156687 | 84982278750 | 917067192 |
| Loss\_Frames | 0 | 0 | 0 | 0 |
| Loss% | 0.0 | 0.0 | 0.0 | 0.0 |